## Union of http://hl7.org/fhir/uv/ips/StructureDefinition/Device-observer-uv-ips and http://hl7.eu/fhir/eps/StructureDefinition/device-eu-eps

This is the set of resources that conform to either of the profiles Device - Performer or Observer (IPS) (http://hl7.org/fhir/uv/ips/StructureDefinition/Device-observer-uv-ips) and Device (EPS) (http://hl7.eu/fhir/eps/StructureDefinition/device-eu-eps). E.g. what you have to deal with if you get resources conforming to one of them

### Structure

Name | Flags | Card. | Type | Description & Constraints Filter: Bindings Constraints Obligations
--- | --- | --- | --- | ---
Device |  | 0..* |  | Item used in healthcare
meta | Σ | 0..1 | Meta | Metadata about the resource
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created
language |  | 0..1 | code | Language of the resource content Binding: ?? (preferred): A human language.
text |  | 0..1 | Narrative | Text summary of the resource, for human interpretation This profile does not constrain the narrative in regard to content, language, or traceability to data elements
contained |  | 0..* | Resource | Contained, inline Resources
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored
identifier | S | 0..* | Identifier | left: Instance identifier; right: Device Identifier
definition |  | 0..1 | Reference(DeviceDefinition) | The reference to the definition for the device
udiCarrier | Σ | 0..* | BackboneElement | left: Unique Device Identifier (UDI) Barcode string; right: Unique Device Identifier (UDI)
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
deviceIdentifier | Σ | 0..1 | string | Mandatory fixed portion of UDI
issuer |  | 0..1 | uri | UDI Issuing Organization
jurisdiction |  | 0..1 | uri | Regional UDI authority
carrierAIDC | Σ | 0..1 | base64Binary | UDI Machine Readable Barcode String
carrierHRF | Σ | 0..1 | string | UDI Human Readable Barcode String
entryType |  | 0..1 | code | barcode | rfid | manual + Binding: ?? (required): Codes to identify how UDI data was entered.
status | ?!Σ | 0..1 | code | active | inactive | entered-in-error | unknown Binding: ?? (required): The availability status of the device.
statusReason |  | 0..* | CodeableConcept | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off Binding: ?? (extensible): The availability status reason of the device.
distinctIdentifier |  | 0..1 | string | The distinct identification string
manufacturer | S | 0..1 | string | left: Name of device manufacturer; right: Device Manufacturer
manufactureDate |  | 0..1 | dateTime | left: Date when the device was made; right: Device Manufacture Date
expirationDate |  | 0..1 | dateTime | left: Date and time of expiry of this device (if applicable); right: Device Expiration Date
lotNumber |  | 0..1 | string | left: Lot number of manufacture; right: Device Lot Number
serialNumber |  | 0..1 | string | left: Serial number assigned by the manufacturer; right: Device Serial Number
deviceName |  | 0..* | BackboneElement | The name of the device as given by the manufacturer
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
name |  | 1..1 | string | left: The name of the device; right: Device Name
type |  | 1..1 | code | udi-label-name | user-friendly-name | patient-reported-name | manufacturer-name | model-name | other Binding: ?? (required): The type of name the device is referred by.
modelNumber | S | 0..1 | string | left: The model number for the device; right: Device Model Number
partNumber |  | 0..1 | string | The part number of the device
type |  | 0..1 | CodeableConcept | left: The kind or type of device; right: Type of device. Preferably valued by using SNOMED CT. The absence of information, or of devices relevant for purpose of this IPS, shall be explicitly stated by using the codes included in the absent-or-unknown-devices-uv-ips value set. Binding: ?? (preferred): Codes to identify medical devices.
specialization |  | 0..* | BackboneElement | The capabilities supported on a device, the standards to which the device conforms for a particular purpose, and used for the communication
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
systemType |  | 1..1 | CodeableConcept | The standard that is used to operate and communicate
version |  | 0..1 | string | The version of the standard that is used to operate and communicate
version |  | 0..* | BackboneElement | The actual design of the device or software version running on the device
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 0..1 | CodeableConcept | The type of the device version
component |  | 0..1 | Identifier | A single component of the device version
value |  | 1..1 | string | left: The version text; right: Device Version
property |  | 0..* | BackboneElement | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 1..1 | CodeableConcept | Code that specifies the property DeviceDefinitionPropetyCode (Extensible)
valueQuantity |  | 0..* | Quantity | Property value as a quantity
valueCode |  | 0..* | CodeableConcept | Property value as a code, e.g., NTP4 (synced to NTP)
patient |  | 0..1 | Reference(Patient) | Patient to whom Device is affixed
owner |  | 0..1 | Reference(Organization) | Organization responsible for device
contact |  | 0..* | ContactPoint | Details for human/organization for support
location |  | 0..1 | Reference(Location) | Where the device is found
url |  | 0..1 | uri | Network address to contact device
note |  | 0..* | Annotation | left: Device notes and comments; right: Device Note
safety | Σ | 0..* | CodeableConcept | Safety Characteristics of Device
parent |  | 0..1 | Reference(Device) | The parent device
Documentation for this format